{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"merged":[[0,1,0,6],[1,1,1,6]]}
[null,"附件四："]
[null,"2019年度六圩污水厂设备设施维修工作计划"]
[null,"序号","设备名称","使用地点","规格型号及功率","厂家","现状"]
[null,1,"1#旋流沉砂池","一期调节池","直径φ3650mm\nXLC1980","江苏天雨","泥沙截留效率低"]
[null,2,"2#旋流沉砂池","一期调节池","直径φ3650mm\nXLC1980","江苏天雨","泥沙截留效率低"]
[null,3,"2#刮吸泥机","一期二沉池","直径φ32m","无锡通用机械厂","已使用13年，累计运行53235小时"]
[null,4,"4#刮吸泥机","一期二沉池","直径φ32m","无锡通用机械厂","已使用13年，累计运行59242小时"]
[null,5,"1#旋流沉砂池","二期进水泵房","SF-320","加拿大爱维","鼓风机损坏"]
[null,6,"1#细格栅","二期细格栅间","GJW/100","无锡科尔","网板开裂，累计运行74316小时"]
[null,7,"2#细格栅","二期细格栅间","GJW/100","无锡科尔","网板开裂，累计运行139531小时"]
[null,8,"3#细格栅","二期细格栅间","GJW/100","无锡科尔","网板开裂，累计运行99755小时"]
[null,9,"5#内回流泵","二期生物池","Q=2100m3/h H=1.5m","青岛海斯特","流量下降严重，累计运行46776小时"]
[null,10,"3#剩余污泥泵","二期生物池","Q=100m³/h H=10m","青岛海斯特","变频器损坏、叶轮磨损严重，累计运行4660小时"]
[null,11,"1#干式离心泵","中水回用泵房","Q=917m3/h，H=30.0m","格兰富","频繁跳停"]
[null,12,"5#干式离心泵","中水回用泵房","Q=917m3/h，H=30.0m","格兰富","频繁跳停"]
[null,13,"1#罗茨风机","一期水解池","Q=18.9Nm3/h H=6.0m","HIBON","待安装"]
[null,14,"2#空压机","砂滤池","Q=7.74m3/min，P=7.5bar","阿特拉斯","已使用8年"]
[null,15,"二期7#进水泵","进水泵房","KRTK 350-420/R1006 UNG-S","KSB","已使用3年"]
[null,16,"二期进水5#泵","进水泵房","KRTK 350-420/1006 UNG-K","KSB","已使用8年"]
[null,17,"三期2#外回流泵","生物池","H12A-SD1+HN030X8-XMSA","青岛海斯特","已使用3年"]
[null,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}